Amplificateur Yamaha

Liste des commandes dans calaos installer

Fonctionne avec la serie rx

Volume X

Power on

Power off

source X

source 1 -> HDMI 1
source 2 -> HDMI 2
source 3 -> HDMI 3
source 4 -> HDMI 4
source 5 -> HDMI 5
source 6 -> Tuner
source 7 -> Phono
source 8-> Video 1
source 9 -> Video 2
source 10 -> Video 3
source 11 -> Video 4
source 12 -> Video 5
source 13 -> Video 6
source 14 -> V-Aux
source 15 -> Audio 1
source 16 -> Audio 2
source 17 -> Dock
source 18 -> iPod
source 19 -> Bluetooth
source 20 -> Network
source 21 -> Napster
source 22 -> Net Radio
source 23 -> USB
source 24-> iPod (USB)
source 25 -> PC
source 26 -> UAW

custom cmd

exemple

custom @MAIN:INP=HDMI1

@MAIN @ZONE2 @ZONE3

Command Details of SubUnit: MAIN
PWR
[PUT Command]
@MAIN:PWR=
[Parameters]
Standby :turining its state to Standby / GET: indicating Standby status.
On :turining its state to On / GET: indicating On status.
On/Standby :toggling its status between On/Standby
SLEEP
[PUT Command]
@MAIN:SLEEP=
[Parameters]
Off :turining its setting state to Off / GET: indicating Off setting status.
30 min :setting to 30 min / GET: indicating it's setting is 30 min.
60 min :setting to 60 min / GET: indicating it's setting is 60 min.
90 min :setting to 90 min / GET: indicating it's setting is 90 min.
120 min :setting to 120 min / GET: indicating it's setting is 120 min.
Last :setting to the value set last
VOL
[PUT Command]
@MAIN:VOL=
[Parameters]
Down :decrementing by 1 step (0.5dB)
Up :incrementing by 1 step (0.5dB)
Down 1 dB :decrementing by 1 dB
Up 1 dB :incrementing by 1 dB
Down 2 dB :decrementing by 2 dB
Up 2 dB :incrementing by 2 dB
Down 5 dB :decrementing by 5 dB
Up 5 dB :incrementing by 5 dB
Numerical Number: -80.5 to 16.5, Step: 0.5 :setting to the specified value.
-80.5 means muting. First decimal place must be always included. Ex: 10.0, -25.0 or 0.0 etc. The unit for this parameter is "dB".
MUTE
[PUT Command]
@MAIN:MUTE=
[Parameters]
Off :turining its state to Off / GET: indicating Off status.
Att -40 dB :attenuating by 40 dB from current volume status. / GET: indicating attenuated by 40 dB from current
volume status.
Att -20 dB :attenuating by 20 dB from current volume status. / GET: indicating attenuated by 20 dB from current
volume status.
On :turining its state to On / GET: indicating On status.
On/Off :toggling its status between On/Off
MAXVOL
[PUT Command]
@MAIN:MAXVOL=
[Parameters]
Numerical Number: -30.0 to 15.0, Step: 5.0 :setting to the specified value. / GET: indicating the current setting value.
First decimal place must be always included. Ex: 10.0, -25.0 or 0.0 etc.
The unit for this parameter is "dB".
16.5: setting to the specified value. / GET: indicating the current setting value.
Meaning no limit of maximum volume
The unit for this parameter is "dB".
INITVOLMODE
[PUT Command]
@MAIN:INITVOLMODE=
[Parameters]
Offturining its setting state to Off / GET: indicating Off setting status.
On :turining its setting state to On / GET: indicating On setting status.
INITVOLLVL
[PUT Command]
@MAIN:INITVOLLVL=
[Parameters]
Mute :turining its setting state to Mute / GET: indicating Mute setting status.
Initially muted when turned on
Numerical Number: -80.0 to 16.5, Step: 0.5
setting to the specified value. / GET: indicating the current setting value.
First decimal place must be always included. Ex: 10.0, -25.0 or 0.0 etc.
The unit for this parameter is "dB".
INP
[PUT Command]
@MAIN:INP=
[Parameters]
SIRIUS :selecting input SIRIUS
TUNER :selecting input TUNER
HDMI1 :selecting input HDMI1
HDMI2 :selecting input HDMI2
HDMI3 :selecting input HDMI3
HDMI4 :selecting input HDMI4
HDMI5 :selecting input HDMI5
AV1 :selecting input AV1
AV2 :selecting input AV2
AV3 :selecting input AV3
AV4 :selecting input AV4
AV5 :selecting input AV5
AV6 :selecting input AV6
V-AUX :selecting input V-AUX
AUDIO1 :selecting input AUDIO1
AUDIO2 :selecting input AUDIO2
DOCK :selecting input DOCK
iPod :selecting input iPod
Bluetooth :selecting input Bluetooth
UAW :selecting input UAW
NET :selecting input NET
Rhapsody :selecting input Rhapsody
SIRIUS InternetRadio :selecting input SIRIUS InternetRadio
Pandora :selecting input Pandora
Napster :selecting input Napster
PC :selecting input PC
NET RADIO :selecting input NET RADIO
USB :selecting input USB
iPod (USB) :selecting input iPod (USB)
DECODERSEL
[PUT Command]
@MAIN:DECODERSEL=
[Parameters]
Auto :turining its setting state to Auto
Automatically selects audio decoder. Default value.
DTS :turining its setting state to DTS
Audio decoder is fixed to DTS
SCENE
[PUT Command]
@MAIN:SCENE=
[Parameters]
Scene 1
selecting Scene 1
Scene 2
selecting Scene 2
Scene 3
selecting Scene 3
Scene 4
selecting Scene 4
SPBASS
[PUT Command]
@MAIN:SPBASS=
[Parameters]
Numerical Number: -6.0 to 6.0, Step: 0.5
setting to the specified value. / GET: indicating the current setting value.
First decimal place must be always included. Ex: 3.0, -4.0
The unit for this parameter is "dB".
SPTREBLE
[PUT Command]
@MAIN:SPTREBLE=
[Parameters]
Parameters are the same as
SPBASS
PUREDIRMODE
[PUT Command]
@MAIN:PUREDIRMODE=
[Parameters]
Off :turining its setting state to Off
On :turining its setting state to On
ADAPTIVEDRC
[PUT Command]
@MAIN:ADAPTIVEDRC=
[Parameters]
Off :turining its setting state to Off
Auto :turining its setting state to Auto
LIPSYNCMODE
[PUT Command]
@MAIN:LIPSYNCMODE=
[Parameters]
Manual :turining its setting state to Manual / GET: indicating Manual setting status.
About "Manual" setting of Lipsync Mode: When selecting "Manual" here, the audio delay value can be
manually set. The effective setting of the audio delay value has some dependencies as follows. In case of
using Analog Video Output only (no HDMI connection is active), audio delay value set by "@MAIN:ANLGOUT"
command is effective. In case that HDMI OUT1 is in active connection, the value set by
"@MAIN:HDMIOUT1MANUAL" command works. Else if HDMI OUT2 is the only one activated, the setting by
"@MAIN:HDMIOUT2MANUAL" is enabled.
Auto :turining its setting state to Auto / GET: indicating Auto setting status.
About Lipsync Mode "Auto": Basically, Audio Delay value has 5 different settings internally according to "Video
Output State (5 Status available)". And the 5 different status of "Video Output State" is determined by the
combination of two states of "Display's state of compatibility/incompatibility with Auto Lipsync feature" and
"Current effective HDMI output state (on the receiver)", which means 4 status, plus a status of "Analog Video
Out only in use", summing up to 5 in total. The "Auto" setting of Lipsync Mode is to dynamically change the
Audio Delay value corresponding to a specific status of Video Output State. "Video Output State" can be
retrieved with a command of "@MAIN:SELINFO", and you can set the effective Audio Delay value according to
respective Video Output status by these commands as following;
When "@MAIN:SELINFO=Analog": the audio delay can be set by "@MAIN:ANLGOUT" command
When "@MAIN:SELINFO=HDMI1 Auto" (meaning TV compatible with Auto Lipsync and HDMI OUT1 is
effective): the audio delay can be set by "@MAIN:HDMIOUT1OFFSET" command
When "@MAIN:SELINFO=HDMI1 Manual" (meaning TV incompatible with Auto Lipsync and HDMI OUT1 is
effective): the audio delay can be set by "@MAIN:HDMIOUT1MANUAL" command
When "@MAIN:SELINFO=HDMI2 Auto" (meaning TV compatible with Auto Lipsync and HDMI OUT 2 is the
only one in effective): the audio delay can be set by "@MAIN:HDMIOUT2OFFSET" command
When "@MAIN:SELINFO=HDMI2 Manual" (meaning TV incompatible with Auto Lipsync and HDMI OUT 2 is
the only one in effective): the audio delay can be set by "@MAIN:HDMIOU21MANUAL" command
LIPSYNCANLGOUT
[PUT Command]
@MAIN:LIPSYNCANLGOUT=
[Parameters]
Down
incrementing by 1 step (1 millisecond)
Up
decrementing by 1 step (1 millisecond)
Numerical Number: 0 to 250, Step: 1
setting to the specified value.
The unit for this parameter is "ms".
LIPSYNCHDMIOUT1OFFSET
[PUT Command]
@MAIN:LIPSYNCHDMIOUT1OFFSET=
[Parameters]
Down
incrementing by 1 step (1 millisecond)
Up
decrementing by 1 step (1 millisecond)
Numerical Number: -250 to 250, Step: 1
setting to the specified value.
The unit for this parameter is "ms".
LIPSYNCHDMIOUT1MANUAL
[PUT Command]
@MAIN:LIPSYNCHDMIOUT1MANUAL=
[Parameters]
Down
incrementing by 1 step (1 millisecond)
Up
decrementing by 1 step (1 millisecond)
Numerical Number: 0 to 250, Step: 1
setting to the specified value.
The unit for this parameter is "ms".
LIPSYNCHDMIOUT2OFFSET
[PUT Command]
@MAIN:LIPSYNCHDMIOUT2OFFSET=
[Parameters]
Parameters are the same as
LIPSYNCHDMIOUT1OFFSET
LIPSYNCHDMIOUT2MANUAL
[PUT Command]
@MAIN:LIPSYNCHDMIOUT2MANUAL=
[Parameters]
Parameters are the same as
LIPSYNCHDMIOUT1MANUAL
HDMIOUT
[PUT Command]
@MAIN:HDMIOUT=
[Parameters]
Off :turining its setting state to Off (output is disabled)/ GET: indicating Off setting status.
OUT :turining its setting state to OUT (meaning output is enabled) / GET: indicating OUT setting status.
Initial Auto Feedback is Available
[Parameters]
Hall in Munich :turining its setting state to Hall in Munich / GET: indicating Hall in Munich setting status.
Hall in Vienna :turining its setting state to Hall in Vienna / GET: indicating Hall in Vienna setting status.
Chamber :turining its setting state to Chamber / GET: indicating Chamber setting status.
Cellar Club :turining its setting state to Cellar Club / GET: indicating Cellar Club setting status.
The Roxy Theatre :turining its setting state to The Roxy Theatre / GET: indicating The Roxy Theatre setting status.
The Bottom Line :turining its setting state to The Bottom Line / GET: indicating The Bottom Line setting status.
Sports :turining its setting state to Sports / GET: indicating Sports setting status.
Action Game :turining its setting state to Action Game / GET: indicating Action Game setting status.
Roleplaying Game :turining its setting state to Roleplaying Game / GET: indicating Roleplaying Game setting status.
Music Video :turining its setting state to Music Video / GET: indicating Music Video setting status.
Standard :turining its setting state to Standard / GET: indicating Standard setting status.
Spectacle :turining its setting state to Spectacle / GET: indicating Spectacle setting status.
Sci-Fi :turining its setting state to Sci-Fi / GET: indicating Sci-Fi setting status.
Adventure :turining its setting state to Adventure / GET: indicating Adventure setting status.
Drama :turining its setting state to Drama / GET: indicating Drama setting status.
Mono Movie :turining its setting state to Mono Movie / GET: indicating Mono Movie setting status.
2ch Stereo :turining its setting state to 2ch Stereo / GET: indicating 2ch Stereo setting status.
7ch Stereo :turining its setting state to 7ch Stereo / GET: indicating 7ch Stereo setting status.
Surround Decoder :turining its setting state to Surround Decoder / GET: indicating Surround Decoder setting status.
ADAPTIVEDSP
[PUT Command]
@MAIN:ADAPTIVEDSP=
[Parameters]
Off :turining its setting state to Off / GET: indicating Off setting status.
Auto :turining its setting state to Auto / GET: indicating Auto setting status.
3DCINEMA
[PUT Command]
@MAIN:3DCINEMA=
Parameter
@MAIN:3DCINEMA=?
Operating & retrieving 3D DSP setting state
[Parameters]
Off :turining its setting state to Off / GET: indicating Off setting status.
Auto :turining its setting state to Auto / GET: indicating Auto setting status.
EXSURDECODER
[PUT Command]
@MAIN:EXSURDECODER=
Parameter
@MAIN:EXSURDECODER=?
Operating & retrieving Extended Surround setting state
[Parameters]
Off :turining its setting state to Off / GET: indicating Off setting status.
Auto :turining its setting state to Auto / GET: indicating Auto setting status.
Dolby PLIIx Movie :turining its setting state to Dolby PLIIx Movie / GET: indicating Dolby PLIIx Movie setting status.
Dolby PLIIx Music :turining its setting state to Dolby PLIIx Music / GET: indicating Dolby PLIIx Music setting status.
EX/ES :turining its setting state to EX/ES / GET: indicating EX/ES setting status.
2CHDECODER
[PUT Command]
@MAIN:2CHDECODER=
[Parameters]
Dolby PL
Dolby PLII Movie :turining its setting state to Dolby PLII Movie / GET: indicating Dolby PLII Movie setting status.
Dolby PLII Music :turining its setting state to Dolby PLII Music / GET: indicating Dolby PLII Music setting status.
Dolby PLII Game :turining its setting state to Dolby PLII Game / GET: indicating Dolby PLII Game setting status.
Dolby PLIIx Movie :turining its setting state to Dolby PLIIx Movie / GET: indicating Dolby PLIIx Movie setting status.
Dolby PLIIx Music :turining its setting state to Dolby PLIIx Music / GET: indicating Dolby PLIIx Music setting status.
Dolby PLIIx Game :turining its setting state to Dolby PLIIx Game / GET: indicating Dolby PLIIx Game setting status.
DTS NEO:6 Cinema :turining its setting state to DTS NEO:6 Cinema / GET: indicating DTS NEO:6 Cinema setting status.
DTS NEO:6 Music :turining its setting state to DTS NEO:6 Music / GET: indicating DTS NEO:6 Music setting status.
PLAYBACK
[PUT Command]
@MAIN:PLAYBACK=
[Parameters]
Stop : change its state to Stop
Pause